

**Paano upang itakda ang Static IP address para sa isang D-Link ™ router network** :

If you will be making incoming iClose-Up connections to one or more iClose-Up computers that are using a D-Link™ router to access the Internet you will need to set up Static IP addresses on the iClose-Up computers. Kung ikaw ay nagsasagawa ng mga papasok na iClose-Up na koneksyon sa isa o higit pang mga iClose-Up na mga computer na gumagamit ng isang D-Link ™ router access ang Internet, kailangan mong i-set up ng Static IP address sa iClose-Up computer. Before we can do this we need to get some information from the router. Bago namin ito na kailangan namin upang makakuha ng ilang impormasyon mula sa router . To do this… Upang gawin ito ...

1. 1. 1.        Open your web browser (on a PC behind your router) and enter the address **192.168.0.1** (the default IP of the router) then press **Enter** . Buksan ang iyong web browser (sa isang PC sa likod ng iyong router) at **ipasok** ang address 192.168.0.1 (ang default IP ng **router)** pagkatapos ay pindutin ang Enter.
2. 2. 2.        Enter the router Administrator **Password** (default is “admin”). Ipasok ang router **Password** Administrator (Ang default ay "admin") .
3. 3. 3.       Write down on a piece of paper the IP Address in the **Primary DNS** field (in our example **4.2.2.1** ). Isulat sa isang piraso ng papel ang mga IP Address sa **Pangunahing** field **ng** DNS (sa aming **halimbawa** 4.2.2.1) .



1. 4. 4.        Click the **DHCP** link at the bottom of the page. **I-click** ang DHCP link sa ibaba ng pahina.
2. 5. 5.        Write down on a piece of paper the name in the **Domain Name** field (in our example **@home** ). Isulat sa isang piraso ng papel ang pangalan sa patlang **ng Pangalan** ng Domain (sa **aming Halimbawa** @ home ).
3. 6. 6.        Close your web browser. Isara ang iyong web browser .



You will now set Static IP addresses on each iClose-Up computer that will be getting incoming iClose-Up connections. Mo na ngayong i-set ng Static IP address sa bawat iClose-Up na computer na nakakakuha ng papasok iClose-Up na koneksyon. If you have only one iClose-Up computer getting incoming connections then just set a Static IP address on that one computer. Kung mayroon kang isa lamang iClose-Up na computer na pagkuha ng mga papasok na koneksyon pagkatapos lamang magtakda ng isang Static IP address na isang computer.

*            If a computer you will be making incoming connections to is a Windows 95/98/Me machine [click here](http://translate.googleusercontent.com/translate_c?hl=tl&prev=/search%3Fq%3Dconfigure%2Bdlink%2Brouter%2Bfor%2BStatic%2BIP.%26hl%3Dtl%26biw%3D990%26bih%3D459%26prmd%3Dimvns&rurl=translate.google.com.ph&sl=en&u=http://www.norton-lambert.com/helpfile/Set%2520static%2520IP%2520for%2520D-Link.htm&usg=ALkJrhgyDwm4VHfOdwayXswjmYvcFgpT0A#win9x) Kung ang isang computer na ikaw ay nagsasagawa ng mga papasok na koneksyon sa ay isang [Windows 95/98/Me machine mag](http://translate.googleusercontent.com/translate_c?hl=tl&prev=/search%3Fq%3Dconfigure%2Bdlink%2Brouter%2Bfor%2BStatic%2BIP.%26hl%3Dtl%26biw%3D990%26bih%3D459%26prmd%3Dimvns&rurl=translate.google.com.ph&sl=en&u=http://www.norton-lambert.com/helpfile/Set%2520static%2520IP%2520for%2520D-Link.htm&usg=ALkJrhgyDwm4VHfOdwayXswjmYvcFgpT0A#win9x) -click dito
*            If a computer you will be making incoming connections to is a Windows NT 4.0 machine [click here](http://translate.googleusercontent.com/translate_c?hl=tl&prev=/search%3Fq%3Dconfigure%2Bdlink%2Brouter%2Bfor%2BStatic%2BIP.%26hl%3Dtl%26biw%3D990%26bih%3D459%26prmd%3Dimvns&rurl=translate.google.com.ph&sl=en&u=http://www.norton-lambert.com/helpfile/Set%2520static%2520IP%2520for%2520D-Link.htm&usg=ALkJrhgyDwm4VHfOdwayXswjmYvcFgpT0A#winnt) Kung ang isang computer na ikaw ay nagsasagawa ng mga papasok na koneksyon sa ay isang Windows [NT 4.0 machine mag](http://translate.googleusercontent.com/translate_c?hl=tl&prev=/search%3Fq%3Dconfigure%2Bdlink%2Brouter%2Bfor%2BStatic%2BIP.%26hl%3Dtl%26biw%3D990%26bih%3D459%26prmd%3Dimvns&rurl=translate.google.com.ph&sl=en&u=http://www.norton-lambert.com/helpfile/Set%2520static%2520IP%2520for%2520D-Link.htm&usg=ALkJrhgyDwm4VHfOdwayXswjmYvcFgpT0A#winnt) -click dito
*            If a computer you will be making incoming connections to is a Windows 2000 or Windows XP machine [click here](http://translate.googleusercontent.com/translate_c?hl=tl&prev=/search%3Fq%3Dconfigure%2Bdlink%2Brouter%2Bfor%2BStatic%2BIP.%26hl%3Dtl%26biw%3D990%26bih%3D459%26prmd%3Dimvns&rurl=translate.google.com.ph&sl=en&u=http://www.norton-lambert.com/helpfile/Set%2520static%2520IP%2520for%2520D-Link.htm&usg=ALkJrhgyDwm4VHfOdwayXswjmYvcFgpT0A#win2k) Kung ang isang computer na ikaw ay nagsasagawa ng mga papasok na koneksyon sa ay isang Windows 2000 o [Windows XP](http://translate.googleusercontent.com/translate_c?hl=tl&prev=/search%3Fq%3Dconfigure%2Bdlink%2Brouter%2Bfor%2BStatic%2BIP.%26hl%3Dtl%26biw%3D990%26bih%3D459%26prmd%3Dimvns&rurl=translate.google.com.ph&sl=en&u=http://www.norton-lambert.com/helpfile/Set%2520static%2520IP%2520for%2520D-Link.htm&usg=ALkJrhgyDwm4VHfOdwayXswjmYvcFgpT0A#win2k) machine click dito

**If the machine you will be making incoming connections to is running Windows 95/98/Me: Kung ang mga makina na ikaw ay paggawa ng mga papasok na koneksyon sa ay nagpapatakbo ng Windows 95/98/Me:**

1. 1. 1.        Go to your Windows desktop and right -click on **Network Neighborhood** or **My Network Places** . Pumunta sa iyong Windows desktop at right-click sa **Kapitbahayan ng** Network **o ang Aking** Network Lugar.
2. 2. 2.        Left -click **Properties** from the drop down menu. Kaliwa-click **ang Properties** mula sa drop down menu.
3. 3. 3.        Select **TCP/IP** for your network adapter . Piliin **ang TCP /** IP para sa iyong network adaptor .
4. 4. 4.        Click on the **Properties** button. Mag-click sa **pindutan** ng Properties.
5. 5. 5.        Click on the following tabs: Mag-click sa sumusunod na mga tab:
6. 1. 1.         Under the **IP Address** tab, set to " **Specify an IP address** ” and set the **IP Address** to **192.168.0.2** " . Sa ilalim ng **IP Address** ng tab, itinakda sa **"Tukuyin ang isang IP** address na" at **itakda ang** IP **Address** sa 192.168.0.2 ". It is recommended that the last part (octet) of each IP address be sequential starting with **2** for the first computer, then if you are setting static IP's on multiple computers, **3** for the next computer, and so on for each computer on your network. Ito ay inirerekumenda na ang huling bahagi (octet) ng bawat IP address ay nanggagalaing simula may **2** para sa ang unang computer, pagkatapos ay kung ikaw ay setting static IP ay sa maramihang mga **computer,** 3 para sa susunod na computer, at iba pa para sa bawat computer sa iyong network .
7. 2. 2.         On the same **IP Address** tab, on the **Subnet Mask** line, set the Subnet Mask to **255.255.255.0** Sa parehong **IP Address** na tab, sa **linya ng** Subnet mask, itakda ang **Subnet** mask 255.255.255.0
8. 3. 3.         Under the **Gateway** tab, enter in a gateway of **192.168.0.1** and press the **Add** button. Sa ilalim ng **tab** ng Gateway, ipasok sa isang **gateway** ng 192.168.0.1 at pindutin **ang** pindutang Idagdag.
9. 4. 4.         Under the **DNS Configuration** tab, select **Enable DNS,** then put in the unique **Host** name for this computer (to find the **Host** name of this computer, right click on the red iClose-Up triangles in the lower right of the screen, select **iClose-Up Main Screen** then select the **Help** pull down menu, then select **View Computer Name** ). Sa ilalim ng **tab ng** Configuration ng **DNS, piliin ang** Paganahin ang DNS, pagkatapos ay **ilagay** sa natatanging pangalan Host para sa computer na **ito** (upang mahanap ang host name ng computer na ito, i-right click sa red iClose-Up triangles sa **ibabang-kanan ng** screen, piliin ang iClose- **Up Main Screen** pagkatapos ay **piliin** ang Tulong sa pull down menu, pagkatapos **ay piliin ang Tingnan** ang Pangalan ng Computer).
10. 5. 5.         Enter the **Domain** name that you got from the router and we had you write down into the **Domain** field, and the **DNS IP** address that you got from the router into the **DNS Server Search Order** field. Ipasok ang **Domain** na pangalan na iyong nakuha mula sa router at kami ay isulat mo sa patlang **na** Domain, at ang **mga DNS** IP address na iyong nakuha mula sa router **sa DNS Server Search** Order patlang . Next press the **Add** button to add the **DNS IP** address we entered to the list box, then Susunod na pindutin ang pindutan ng **Magdagdag ng** button upang idagdag ang **DNS IP** address namin ipinasok sa listahan ang kahon, at pagkatapos ay click **OK** . click ang **OK.** Click **OK** again to close the Network window and restart your computer for the changes to take effect. **I-click** ang OK muli upang isara ang window ng Network at i-restart ang iyong computer para sa mga pagbabago na umepekto. After you set Static IP addresses on each iClose-Up computer that will be getting incoming iClose-Up connections you should go back and start at the beginning of this Router help section again. Matapos mong itakda ang Static IP address sa bawat iClose-Up na computer na nakakakuha papasok iClose-Up koneksyon dapat mong bumalik at magsimula sa umpisa ng seksyon na ito ng tulong ng router muli. This time you would follow the directions knowing you are using Static IP addresses. Oras na ito nais mong sundin ang mga direksyon na alam mo ginagamit ang Static IP address. You can rerun the Help file and in the table of **Contents** go to the [**Routers**](http://translate.googleusercontent.com/translate_c?hl=tl&prev=/search%3Fq%3Dconfigure%2Bdlink%2Brouter%2Bfor%2BStatic%2BIP.%26hl%3Dtl%26biw%3D990%26bih%3D459%26prmd%3Dimvns&rurl=translate.google.com.ph&sl=en&u=http://www.norton-lambert.com/helpfile/Routers.htm&usg=ALkJrhgGzMhe-Ha9nzvF2gN9tNnFcXg8MA) section. Maaari mong muling palabas ng pelikula ang Help file at sa table ng mga **Nilalaman** sa [**Routers**](http://translate.googleusercontent.com/translate_c?hl=tl&prev=/search%3Fq%3Dconfigure%2Bdlink%2Brouter%2Bfor%2BStatic%2BIP.%26hl%3Dtl%26biw%3D990%26bih%3D459%26prmd%3Dimvns&rurl=translate.google.com.ph&sl=en&u=http://www.norton-lambert.com/helpfile/Routers.htm&usg=ALkJrhgGzMhe-Ha9nzvF2gN9tNnFcXg8MA) seksyon.

**If the machine you will be making incoming connections to is running Windows NT 4.0: Kung ang makina ang ikaw ay paggawa ng mga papasok na koneksyon sa ay nagpapatakbo ng Windows NT 4.0:**

1. 1. 1.        Go to your Windows desktop and right -click on **Network Neighborhood** . Pumunta sa iyong Windows desktop at right-click sa **Network Kapitbahayan.**
2. 2. 2.        Left -click **Properties** . Kaliwa-click **Properties.**
3. 3. 3.        Select the **Protocols** tab. Piliin ang tab **na** Mga protocol.
4. 4. 4.        Highlight **TCP/IP Protocol** . I-highlight **ang TCP / IP** Protocol .
5. 5. 5.        Click on the **Properties** button. Mag-click sa **pindutan** ng Properties.
6. 6. 6.        Select **Specify an IP address** . Piliin **ang Tukuyin ang isang IP** address .
7. 1. 1.         Enter the **IP Address** of **192.168.0.2** ” . Ipasok ang **IP Address** ng **192.168.0.2** ". Remember it is recommended that the last part (octet) of each IP address be sequential starting with **2** for the first computer, then if you are setting static IP's on multiple computers, **3** for the next computer, and so on for each computer on your network. Tandaan inirerekomenda na ang huling bahagi (octet) ng bawat IP address ay nanggagalaing simula may **2** para sa ang unang computer, pagkatapos kung ka ay setting static IP ay sa maraming mga **computer,** 3 para sa susunod na computer, at iba pa para sa bawat computer sa iyong network.
8. 2. 2.         On the same **IP Address** tab, on the **Subnet Mask** line, set the Subnet Mask to **255.255.255.0** Sa parehong **IP Address** na tab, sa **linya ng** Subnet mask, itakda ang **Subnet** mask 255.255.255.0
9. 3. 3.         On the same **IP Address** tab, on the **Default Gateway** line, enter in a default gateway of **192.168.0.1** Sa parehong **IP Address** na tab, sa **linya ng** Default Gateway, ipasok sa isang default **gateway** ng 192.168.0.1
10. 4. 4.         Select the **DNS** tab. Piliin ang tab **na** DNS . E nter the unique **Host Name** for this computer (to find the **Host** name of this computer, right click on the red iClose-Up triangles in the lower right of the screen, select **iClose-Up Main Screen** then select the **Help** pull down menu, then select **View Computer Name** ). E nter natatanging **Pangalan ng Host** para sa computer na ito (upang mahanap **ang** Host pangalan ng computer na ito, i-right click ang pulang iClose-Up triangles sa ibabang-kanan ng screen, **piliin ang iClose-Up** Main Screen pagkatapos ay **piliin** ang Tulong sa pull down menu, pagkatapos ay piliin ang **Tingnan Computer Pangalan).**
11. 5. 5.         Enter the **Domain** name you got from the router and we had you write down in the **Domain** field Ipasok ang pangalan **ng** Domain na nakuha mo mula sa router at kami ay isulat mo sa **patlang** na Domain
12. 6. 6.         Next click the **Add** button in the **DNS Service Search Order** box, enter the **DNS IP** address you got from the router and we had you write down, into the new **TCP/IP DNS Server** window, then click **Add** . Susunod na i-click **ang** Magdagdag ng button sa **ang kahon ng DNS** Serbisyo Search **Order, ipasok** ang DNS IP address na ba kayong mula sa router at kami ay isulat **mo, sa ang bagong TCP** / IP DNS Server **window, at** pagkatapos ay i-click ang Idagdag. Click **OK** , then click **OK** again and restart your computer for the changes to take effect. I-click ang **OK,** at pagkatapos ay i-click ang **OK** muli at i-restart ang iyong computer para sa mga pagbabago na umepekto. After you set Static IP addresses on each iClose-Up computer that will be getting incoming iClose-Up connections you should go back and start at the beginning of this Router help section again. Matapos mong itakda ang Static IP address sa bawat iClose-Up na computer na nakakakuha papasok iClose-Up koneksyon dapat mong bumalik at magsimula sa umpisa ng seksyon na ito ng tulong ng router muli. This time you would follow the directions knowing you are using Static IP addresses. Oras na ito nais mong sundin ang mga direksyon na alam mo ginagamit ang Static IP address. You can rerun the Help file and in the table of **Contents** go to the [**Routers**](http://translate.googleusercontent.com/translate_c?hl=tl&prev=/search%3Fq%3Dconfigure%2Bdlink%2Brouter%2Bfor%2BStatic%2BIP.%26hl%3Dtl%26biw%3D990%26bih%3D459%26prmd%3Dimvns&rurl=translate.google.com.ph&sl=en&u=http://www.norton-lambert.com/helpfile/Routers.htm&usg=ALkJrhgGzMhe-Ha9nzvF2gN9tNnFcXg8MA) section. Maaari mong muling palabas ng pelikula ang Help file at sa table ng mga **Nilalaman** sa [**Routers**](http://translate.googleusercontent.com/translate_c?hl=tl&prev=/search%3Fq%3Dconfigure%2Bdlink%2Brouter%2Bfor%2BStatic%2BIP.%26hl%3Dtl%26biw%3D990%26bih%3D459%26prmd%3Dimvns&rurl=translate.google.com.ph&sl=en&u=http://www.norton-lambert.com/helpfile/Routers.htm&usg=ALkJrhgGzMhe-Ha9nzvF2gN9tNnFcXg8MA) seksyon.

**If the machine you will be making incoming connections to is running Windows 2000 or Windows XP: Kung ang mga makina na ikaw ay paggawa ng mga papasok na koneksyon sa ay nagpapatakbo ng Windows 2000 o Windows XP:**

1. 1. 1.         Go to your Windows desktop, or if you are using Windows XP START menu, click START then right -click on **My Network Places** . Pumunta sa iyong Windows desktop, o kung ikaw ay gumagamit ng START menu ng Windows XP, i-click ang START **pagkatapos-right-click** sa Aking mga Lugar sa Network.
2. 2. 2.         Left -click **Properties** . Kaliwa-click **Properties.**
3. 3. 3.         Right -click on **Local Area Connection** . Right-click sa **Local Area Connection.**
4. 4. 4.         Left -click **Properties** . Kaliwa-click **Properties.**
5. 5. 5.         Highlight **Internet Protocol (TCP/IP)** . I-highlight ang **Internet Protocol (TCP / IP).**
6. 6. 6.         Click on the **Properties** button. Mag-click sa **pindutan** ng Properties.
7. 7. 7.         Select **Use the following IP addresses** . Piliin **ang Gamitin ang sumusunod na** mga IP address.
8. 1. 1.         Set the **IP Address** to **192.168.0.2** " . Itakda ang **IP Address 192.168.0.2** ". Remember it is recommended that the last part (octet) of each IP address be sequential starting with **2** for the first computer, then if you are setting static IP's on multiple computers, **3** for the next computer, and so on for each computer on your network. Tandaan inirerekomenda na ang huling bahagi (octet) ng bawat IP address ay nanggagalaing simula may **2** para sa ang unang computer, pagkatapos kung ka ay setting static IP ay sa maraming mga **computer,** 3 para sa susunod na computer, at iba pa para sa bawat computer sa iyong network.
9. 2. 2.         On the **Subnet Mask** line, set the Subnet Mask to **255.255.255.0** Sa linya **ng Subnet** mask, itakda ang Subnet **mask** 255.255.255.0
10. 3. 3.         On the **Default Gateway** line, enter in a default gateway of **192.168.0.1** Sa linya **ng Default** Gateway, ipasok sa isang default gateway **ng** 192.168.0.1
11. 4. 4.         Enter the **DNS IP** address you got from the router and we had you write down in the **Preferred DNS server** line. Ipasok ang **DNS IP** address na ba kayong mula sa router at kami ay isulat mo **sa Preferred DNS** server line .
12. 5. 5.         Click the **Advanced** button. I-click ang **Advanced** na pindutan .
13. 6. 6.         Click the **DNS** tab. I-click ang tab **na** DNS .
14. 7. 7.         Enter the **Domain Name** you got from the router and we had you write down into the **DNS Suffix for this connection** field. Ipasok ang **Domain Name** na nakuha mo mula sa router at kami ay isulat mo sa **ang DNS Suffix para sa koneksyon sa** patlang na ito .
15. 8. 8.         Click **OK** three times to return to the **Network and Dial-Up connections** window then close it. **I-click** ang OK tatlong beses **upang bumalik sa Network at Dial-Up** koneksyon window pagkatapos isara ito. After you set Static IP addresses on each iClose-Up computer that will be getting incoming iClose-Up connections you should go back and start at the beginning of this Router help section again. Matapos mong itakda ang Static IP address sa bawat iClose-Up na computer na nakakakuha papasok iClose-Up koneksyon dapat mong bumalik at magsimula sa umpisa ng seksyon na ito ng tulong ng router muli. This time you would follow the directions knowing you are using Static IP addresses. Oras na ito nais mong sundin ang mga direksyon na alam mo ginagamit ang Static IP address. You can rerun the Help file and in the table of **Contents** go to the [**Routers**](http://translate.googleusercontent.com/translate_c?hl=tl&prev=/search%3Fq%3Dconfigure%2Bdlink%2Brouter%2Bfor%2BStatic%2BIP.%26hl%3Dtl%26biw%3D990%26bih%3D459%26prmd%3Dimvns&rurl=translate.google.com.ph&sl=en&u=http://www.norton-lambert.com/helpfile/Routers.htm&usg=ALkJrhgGzMhe-Ha9nzvF2gN9tNnFcXg8MA) section. Maaari mong muling palabas ng pelikula ang Help file at sa table ng mga **Nilalaman** sa [**Routers**](http://translate.googleusercontent.com/translate_c?hl=tl&prev=/search%3Fq%3Dconfigure%2Bdlink%2Brouter%2Bfor%2BStatic%2BIP.%26hl%3Dtl%26biw%3D990%26bih%3D459%26prmd%3Dimvns&rurl=translate.google.com.ph&sl=en&u=http://www.norton-lambert.com/helpfile/Routers.htm&usg=ALkJrhgGzMhe-Ha9nzvF2gN9tNnFcXg8MA) seksyon.